**Bruneau River (directly below South Side Canal Diversion)**

Pros                                                                                       Cons

More remote location (less vandalism)                  4 miles upstream of CJ Strike Res (might miss some spring inflow & returns)

Stable cross section (contained by banks)             Wider & flatter cross section (small change in stage = larger error in flow)

Possible to measure and estimate higher flow                   Unstable control -> new rating each year

**Bruneau River (below HWY 51 bridge)**

Pros                                                                                       Cons

1.5 miles above CJ Strike Reservoir                          Visible from HWY 51 (more traffic)

Stable cross section (contained by banks)             crosses under HWY at 3 locations (only valid < ~600cfs)

Narrower cross section                                              Unstable control -> new rating each year

                                                                                       Steeper channel slope